<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="74.6" y2="0" width="0" layer="20"/>
<wire x1="74.6" y1="0" x2="74.6" y2="25.39" width="0" layer="20"/>
<wire x1="74.6" y1="25.39" x2="0" y2="25.39" width="0" layer="20"/>
<wire x1="0" y1="25.39" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="ec12_rgb_encoder">
<packages>
<package name="EC12_RGB">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="con-harting-ml">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML20">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CENTER" library="ec12_rgb_encoder" package="EC12_RGB" value="EC12_RGB"/>
<element name="SIDE" library="ec12_rgb_encoder" package="EC12_RGB" value="EC12_RGB"/>
<element name="U$3" library="SparkFun" package="STAND-OFF" value=""/>
<element name="U$4" library="SparkFun" package="STAND-OFF" value=""/>
<element name="U$5" library="SparkFun" package="STAND-OFF" value=""/>
<element name="U$6" library="SparkFun" package="STAND-OFF" value=""/>
<element name="MAIN_CON" library="con-harting-ml" package="ML20" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$14">
<contactref element="CENTER" pad="COMMON"/>
<contactref element="MAIN_CON" pad="12"/>
</signal>
<signal name="N$6">
<contactref element="SIDE" pad="BLUE"/>
<contactref element="MAIN_CON" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="SIDE" pad="BUTTON"/>
<contactref element="MAIN_CON" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="SIDE" pad="GREEN"/>
<contactref element="MAIN_CON" pad="8"/>
</signal>
<signal name="N$11">
<contactref element="SIDE" pad="RED"/>
<contactref element="MAIN_CON" pad="10"/>
</signal>
<signal name="N$13">
<contactref element="CENTER" pad="RED"/>
<contactref element="MAIN_CON" pad="20"/>
</signal>
<signal name="N$17">
<contactref element="CENTER" pad="GREEN"/>
<contactref element="MAIN_CON" pad="18"/>
</signal>
<signal name="N$18">
<contactref element="CENTER" pad="BUTTON"/>
<contactref element="MAIN_CON" pad="16"/>
</signal>
<signal name="N$19">
<contactref element="CENTER" pad="BLUE"/>
<contactref element="MAIN_CON" pad="14"/>
</signal>
<signal name="N$21">
<contactref element="CENTER" pad="B"/>
<contactref element="MAIN_CON" pad="15"/>
</signal>
<signal name="N$22">
<contactref element="SIDE" pad="B"/>
<contactref element="MAIN_CON" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="SIDE" pad="A"/>
<contactref element="MAIN_CON" pad="5"/>
</signal>
<signal name="N$40">
<contactref element="SIDE" pad="COMMON"/>
<contactref element="MAIN_CON" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="CENTER" pad="A"/>
<contactref element="MAIN_CON" pad="19"/>
</signal>
<signal name="N$2">
<contactref element="MAIN_CON" pad="17"/>
<contactref element="CENTER" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="MAIN_CON" pad="3"/>
<contactref element="SIDE" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
